{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":7,"rows_kept":3,"merged":[[0,0,0,6],[3,0,3,4]]}
["里建校区电力实训基地配电网自动化实训场地面硬化工程量清单"]
["序号","单项名称","项目特征及描述","工程量","单位","单价（元）","合计（元）"]
[1,"配电网自动化实训场地地面硬化","配电网自动化实训场地地面硬化处理，需原地面平整，多余碎石挖运到指定区并平整，夯实密实度≥95%，100mm厚C15素砼，每6米宽设6mm宽伸缩缝、沥青填缝，稍高出地面，形成四周排水，工程包含场地内井盖抬升等场地处理内容。",1780.82,"㎡"]