{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["订单"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"订单","index":0,"n_rows":54,"n_cols":12,"rows_kept":54,"merged":[[2,0,2,11],[3,0,3,11],[4,0,5,0],[4,1,5,1],[4,2,4,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[4,8,5,8],[4,9,5,9],[4,10,5,10],[4,11,5,11],[6,7,8,7],[9,7,30,7],[31,7,37,7],[52,0,52,11],[53,0,53,11]],"flags":["formulas_cached_only"]}
[]
[]
["广西水利电力职业技术学院长堽、里建校区建筑楼防火门更换安装清单"]
[]
["产品名称","楼层编号","规  格 (mm)",null,"数量","级别","型式","颜色/面板","面积（㎡）","单价（元）","金额    （元）","备注"]
[null,null,"宽","高"]
["钢质防火门","长堽水电实训楼1F01",1960,2070,1,"乙级","双开",null,{"v":4.0572,"d":"4.06"}]
["钢质防火门","长堽水电实训楼1F02",1980,2070,1,"乙级","双开",null,{"v":4.0986,"d":"4.10"}]
["钢质防火门","长堽水电实训楼2F01",1960,2070,1,"乙级","双开",null,{"v":4.1,"d":"4.10"}]
["钢质防火门","长堽水电实训楼2F02",1980,2110,1,"乙级","双开","黄色平光XJ2011平光（10019），",{"v":4.1778,"d":"4.18"}]
["钢质防火门","长堽水电实训楼3F01",1950,2050,1,"乙级","双开",null,{"v":3.9975,"d":"4.00"}]
["钢质防火门","长堽水电实训楼3F02",1960,2070,1,"乙级","双开",null,{"v":4.0572,"d":"4.06"}]
["钢质防火门","长堽水电实训楼4F01",1960,2110,1,"乙级","双开",null,{"v":4.1356,"d":"4.14"}]
["钢质防火门","长堽水电实训楼4F02",1960,2100,1,"乙级","双开",null,{"v":4.116,"d":"4.12"}]
["钢质防火门","长堽水电实训楼5F01",1960,2110,1,"乙级","双开",null,{"v":4.1356,"d":"4.14"}]
["钢质防火门","长堽水电实训楼5F02",1960,2130,1,"乙级","双开",null,{"v":4.1748,"d":"4.17"}]
["钢质防火门","里建实训楼C6区天面01",1960,2110,1,"乙级","双开",null,4.17]
["钢质防火门","里建实训楼C6区天面02",1975,2070,1,"乙级","双开",null,4.18]
["钢质防火门","里建实训楼A6区天面01",1975,2020,1,"乙级","双开",null,{"v":3.9895,"d":"3.99"}]
["钢质防火门","里建实训楼A6区天面02",1970,2050,1,"乙级","双开",null,{"v":4.0385,"d":"4.04"}]
["钢质防火门","里建实训楼C2区F02",760,1740,1,"乙级","双开",null,{"v":1.3224,"d":"1.32"}]
["钢质防火门","里建实训楼C3区F02",780,1740,1,"乙级","双开",null,{"v":1.3572,"d":"1.36"}]
["钢质防火门","里建实训楼A3区F01",800,1750,1,"乙级","双开",null,{"v":1.4,"d":"1.40"}]
["钢质防火门","里建实训楼C4区F02",760,1760,1,"乙级","双开",null,{"v":1.3376,"d":"1.34"}]
["钢质防火门","里建实训楼B6区F01",1955,2080,1,"乙级","双开",null,{"v":4.0664,"d":"4.07"}]
["钢质防火门","里建实训楼B6区F02",780,1770,1,"乙级","双开",null,{"v":1.3806,"d":"1.38"}]
["钢质防火门","里建实训楼C4区F01",780,1770,1,"乙级","双开",null,{"v":1.3806,"d":"1.38"}]
["钢质防火门","里建实训楼C5区F01",1955,2050,1,"乙级","双开",null,{"v":4.00775,"d":"4.01"}]
["钢质防火门","里建实训楼C5区F02",770,1750,1,"乙级","双开",null,{"v":1.3475,"d":"1.35"}]
["钢质防火门","学生公寓磬园9栋1区F01",760,1760,1,"乙级","双开",null,1.34]
["钢质防火门","学生公寓磬园9栋1区F02",760,1800,1,"乙级","双开",null,{"v":1.368,"d":"1.37"}]
["钢质防火门","学生公寓磬园9栋2区F01",760,1795,1,"乙级","双开",null,{"v":1.3642,"d":"1.36"}]
["钢质防火门","学生公寓磬园9栋2区F01",1975,2090,1,"乙级","双开",null,{"v":4.12775,"d":"4.13"}]
["钢质防火门","学生公寓磬园10栋1区F01",760,1730,1,"乙级","双开",null,{"v":1.3148,"d":"1.31"}]
["钢质防火门","学生公寓磬园10栋1区F02",760,1740,1,"乙级","双开",null,{"v":1.3224,"d":"1.32"}]
["钢质防火门","学生公寓磬园10栋2区F01",1955,2060,1,"乙级","双开",null,{"v":4.0273,"d":"4.03"}]
["钢质防火门","学生公寓磬园10栋2区F02",1965,2090,1,"乙级","双开",null,{"v":4.10685,"d":"4.11"}]
["钢质防火门","学生公寓磬园4栋1区F01",1975,2070,1,"乙级","双开",null,4.12]
["钢质防火门","长堽学生公寓珠江阁1F02",1450,2090,1,"乙级","双开",null,3.03]
["钢质防火门","长堽学生公寓珠江阁1F02",1450,2070,1,"乙级","双开",null,{"v":3,"d":"3.00"}]
["钢质防火门","长堽学生公寓珠江阁1F02",1460,2040,1,"乙级","双开",null,{"v":3,"d":"3.00"}]
["钢质防火门","长堽学生公寓珠江阁1F02",1450,2070,1,"乙级","双开",null,{"v":3,"d":"3.00"}]
["钢质防火门","长堽学生公寓珠江阁1F02",1460,2060,1,"乙级","双开",null,3.01]
["钢质防火门","长堽学生公寓珠江阁1F02",1450,2060,1,"乙级","双开",null,2.99]
["钢质防火门","长堽学生公寓珠江阁1F02",1440,2030,1,"乙级","双开",null,3.03]
["钢质防火门","长堽学生公寓珠江阁1F02",1560,2070,1,"乙级","双开",null,3.23]
["钢质防火门","长堽学生公寓珠江阁1F02",1460,2030,1,"乙级","双开",null,2.96]
["钢质防火门","长堽学生公寓珠江阁1F02",1450,2030,1,"乙级","双开",null,2.94]
["钢质防火门","长堽学生公寓珠江阁1F02",770,1870,1,"乙级","双开",null,1.44]
["钢质防火门","长堽学生公寓珠江阁1F02",770,1860,1,"乙级","双开",null,1.44]
[]
["合计",{"$nulls":3},44,{"$nulls":3},{"v":131.18965,"d":"131.19"}]
["防火门安装要求：防火等级：乙级。其中：门框钢板厚度为1.2mm，门扇钢板厚度为0.8mm，防火板的岩棉板厚度不小于46mm，防火门门扇厚度应≥48mm。"]
["单价含防火门旧门拆除、防火门材料费、安装费、搬运费、消防门框水泥灌浆、税金（普通增值税发票）、墙体恢复、垃圾清理等费用。投标时必须提供翰达消防门的合格证、消防产品流向证明书消防产品认证证书、检测报告（加盖原厂公章，否则竞标无效）。"]