{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":9,"rows_kept":12,"merged":[[0,0,0,8],[9,0,9,5],[9,6,9,7],[11,0,11,8],[12,0,12,8],[13,0,13,8]],"flags":["formulas_cached_only"]}
["电力工程学院实训场所内涵建设采购清单"]
["序号","项目","工艺","规 格","单位","数量","单价（元）","合计（元）","备注"]
[1,"发展历程文化墙","12mmPVC字烤漆+12mmPVC造型底+表晶板UV面层，叠层或错层方式呈现效果","1800mm*2500mm ","平方米",4.5]
[2,"依标准说职业专栏","不锈钢方通骨架底封9mm阻燃板+铝塑板饰面，四周包不锈钢包框；安装位置背后玻璃贴磨砂玻璃膜。","1450mm*7300mm ","平方米",10.58]
[3,"路沿石警示线","拆除20m不锈钢围栏，用丙烯酸户外油漆喷涂路沿石警示线","100mm*9000mm ","项",1]
[4,"依标准说职业不锈钢宣传栏","不锈钢圆立柱、不锈钢方通骨架底封铝塑板饰面，四周包不锈钢包框；","1800mm*2440mm ","块",2]
[5,"供用电技术国家级生产性实训基地","原石材全部拆除，更换12mm仿大理石纹瓷砖，1.2米*4.2斜面阴刻内容，含拆除清理。","1200mm*4200mm*2380mm高","项",1]
[6,"主控楼楼顶字更换","20mmPVC字烤漆+3mm铝塑板面层","字高800mm 16个字","m",12.8]
[7,"景观小品","基础采用螺杆、钢板结构，开挖基坑回填砼；景观造型采用12mmmPVC切割成造型，通过烤漆工艺上色；部分字体、板块底板采用20mmPVC切割烤漆工艺。","3200mm*2200mm ","座",4]
["合计（元）："]
[]
["报价公司（公司名称）：                                                                      联系人：                         联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}