{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"merged":[[0,0,0,6],[15,0,15,5],[17,0,17,2],[17,4,17,5]],"flags":["formulas_cached_only"]}
["自动化工程学院特种作业操作证（低压电工）培训耗材购置清单"]
["序号","货物或\n项目名称","参考品牌型号规格或配置技术参数","数量","计量单位","单价（元）","金额\n（元）"]
[1,"三相电动机","JW-6314，额定电压380V，带连接线\n内置防雷模块：\n1、输入电压频率：47-63Hz/AC浪涌电流：冷启动50A/230VAC\n2、线性调整率（满载）：≤0.5%/输出过载保护：110%-150%hiccup-auto-recovery上升，保持时间：50mS,20mSatfullload(typical)\n3、绝缘强度：I/P-O/P,I/P-FG:1.5KVAC,O/P-FG:0.5KVAC,1min/工作温度：-30~40℃@100%,60℃@60%load\n4、“等电位”功能需出具证明此项功能的第三方具备CMA资质的检验机构证明，竞标文件中提供检测报告复印件\n5、投标文件中提供安全关键件清单截图。\n6、投标文件中提供接地端子标识及滤波电路截图。",10,"台"]
[2,"低压验电器","GDY型0.4kV袖珍型高低压验电器",20,"个"]
[3,"护目眼镜","霍尼韦尔护目镜，VisiOTG-A 100002，透明防雾镜片，规格：宽度158mm，高度：57mm，镜腿长度：131mm，可搭配近视眼镜",20,"副"]
[4,"电工安全标示牌（1批）","定制，规格20*30cm，PVC材质，一套10张",2,"套"]
[5,"电工安全标示挂画（1批）","定制，规格40*60cm，KT板，一套6张",2,"套"]
[6,"保护手套","3M舒适性防滑耐磨手套",20,"对"]
[7,"接地电阻测试仪","ZC29B-2，0-100Ω，塑料外壳，支持物联网SAAS项目的新建并支持授权API的自动生成功能；（投标时需提供该功能截图）",10,"个"]
[8,"钳形电流表","数字型钳形电流表，ZTY0203A",10,"个"]
[9,"按钮盒","NP2-E3001",200,"个"]
[10,"灯座","E27螺口灯座，明装86型",200,"个"]
[11,"电压表","三相导轨式，检测电压AC50V-500V/50-60Hz，导轨固定，测量精度0.5级",200,"个"]
[12,"电流表","导轨式三相电流表，测量精度±2%，测量范围1-100A，频率兼容范围50-60Hz，输入电压AC220V-380V，数显式",200,"个"]
[13,"电流互感器","LMK-0.66，0.5级，150/5，30型，导轨式安装",200,"个"]
["合计（元）："]
[]
["报价公司（公司名称）：",{"$nulls":3},"联系人：",null,null,"联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}