{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":8,"rows_kept":6,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["PE管液压热熔机63-160 液压高配采购清单"]
["序号","名称","规格参数","数量","单位","单价","合价","备注"]
[1,"定制型液压高分子管道熔接装置","加工能力不低于50mm、63mm、75mm、90mm、110mm、125mm、140mm、160m口径的有机高分管材；\n每套包含：\n▲1、高配液压站：能检测故障的电能表（为保证完整合法的知识产权报价中所用电能表需出具专利证书文件佐证）；带LED调节型定时器，LED数显调节型温控仪，工业航空插座；双向进程操纵杆，阻尼连续性调压阀，单向线性泄压阀，机械指针油压表；\n2、实心加热板：铝合金材质电热丝加热板，采用双层进口特氟龙涂层三防不粘黏涂层，AC220V 五线制航空接头，具备连接液压箱的单独控温系统，双色数字显示控温，加热板可调温度不小于0~300℃；\n3、大功率铣刀：16A高功率电极，内嵌式刀盘,刀盘采用高韧度技术,功率大转速快,削切稳定,发热低；\n▲4、机架：抗震双H型回型管结构，配置不锈钢双向单爪性油缸，配置不小于40MM瓦夹；\n5、提篮：四爪双工提篮；",4,"套"]
[2,null,"合计"]
[]
[null,null,"报价公司（公司名称）：",null,null,"联系人：",null,"联系电话："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}