{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":61,"n_cols":9,"rows_kept":61,"merged":[[0,0,0,8],[2,0,2,8],[45,0,45,6],[45,7,45,8],[46,0,46,8],[57,0,57,6],[57,7,57,8],[59,0,59,6],[59,7,59,8],[60,0,60,2],[60,4,60,5],[60,7,60,8]]}
["办公用品采购清单"]
["序号","货物名称","品牌及规格型号","规格参数","单位","数量","单价（元）","合计（元）","图片"]
["一、耗材采购信息（“双带头人”工作室耗材）"]
[1,"电线（红色）","BVR-0.3 m㎡ JB/T8734.4-2012",null,"卷",25]
[2,"电线（红色）","BVR-0.75 m㎡",null,"卷",6]
[3,"电线（红色）","BVR-2.5 m㎡",null,"卷",1]
[4,"电线（黑色）","BVR-0.75 m㎡",null,"卷",3]
[5,"电线（黑色）","BVR-2.5 m㎡",null,"卷",1]
[6,"电线（蓝色）","BVR-0.3 m㎡ JB/T8734.4-2012",null,"卷",25]
[7,"电线（白色）","BVR-0.3 m㎡ JB/T8734.4-2012",null,"卷",25]
[8,"电线（黄绿色，PE线）","BVR-0.75 m㎡",null,"卷",3]
[9,"双芯屏蔽线","2×0.3mm2",null,"米",100]
[10,"压接头","叉型：￠1.25-3 1000个/包\n紫铜材质，接缝电镀",null,"包",30]
[11,"压接头","管型0.5 预绝缘E0508,1000个/包",null,"包",25]
[12,"压接头","管型1.0 预绝缘E1008,1000个/包",null,"包",5]
[13,"压接头","管型2.5 预绝缘E2508,1000个/包",null,"包",5]
[14,"绝缘电工胶带","黑色",null,"个",30]
[15,"白色号码管",null,null,"套",10]
[16,"DB9 公头",null,null,"个",100]
[17,"DB9 母头",null,null,"个",100]
[18,"RS232串口壳",null,null,"个",50]
[19,"场效应管","IRF 740",null,"个",20]
[20,"西门子V20变频器控制模块","6SL3210-5BB13-7UV1主控模块",null,"个",1]
[21,"西门子V20变频器显示面板","6SL3210-5BB13-7UV1显示面板",null,"个",1]
[22,"继电器+底座","继电器：MY4N-G  DC24V \n底座：PYF14A-E，14脚",null,"套",50]
[23,"2020工业铝型材配件套件","1个垫片（内径6mm,外径10mm）、\n3个不锈钢内六角螺丝（M4*10mm、M4*20mm和M5*15mm)、\n1个不锈钢T头螺母（20-M4）",null,"套",50]
[24,"串口网关机体","8路串口232/485转以太网\n实现串口到以太网口的数据的双向透明传输",null,"个",1]
[25,"工业以太网交换机","8口千兆，POE供电",null,"个",1]
[26,"千兆网线","300米盘，0.58无氧铜",null,"个",1]
[27,"水晶头","超五类，RJ45，100个/盒",null,"个",30]
[28,"电源","500W",null,"套",3]
[29,"散热器",null,null,"盒",3]
[30,"工业级热风枪","2000W，温控开关，数显，可调温度，含风嘴3个",null,"把",1]
[31,"热缩管","黑色，3MM，200米/卷",null,"卷",2]
[32,"热缩管","黑色，2.5MM，200米/卷",null,"卷",2]
[33,"PLC-200smart CPU主控电路板","西门子PLC-200smart CPU  SR40 AC/DC/RLY 主控电路板",null,"个",1]
[34,"PLC-200smart CPU输入输出接线模块","西门子PLC-200smart CPU  SR40 AC/DC/RLY 输入输出接线模块",null,"个",1]
[35,"PLC-200smart CPU机体外壳","西门子PLC-200smart CPU  SR40 AC/DC/RLY 机体外壳",null,"个",1]
[36,"音响线","2芯0.75平方100米",null,"条",5]
[37,"PLCUSB-PPI编程电缆","西门子PLC-200smart USB-PPI，黑色，AMSAMOTION，4.7米",null,"个",1]
[38,"组装平台",null,null,"个",1]
[39,"六臂伸缩旋转电视支架","型号:FS503-L；材质:优质冷轧钢；参考尺寸:32-49寸；",null,"个",3]
[40,"终端显示控制与接口部件","小米电视ES43（2022）43寸配套处理器",null,"套",2]
[41,"绿联HDMI一进四出分配器","HDMI分配器\n一进四出；型号：40202；外壳：全金属；接口∶镀镍；分辨率：4K；刷新率：30Hz；配件:5V/1A电源。",null,"个",2]
[42,"绿联hdmi2.0线","长度：30米；分辨率：1080P/60HZ；带宽：4.95Gbps；版本：1.2；线径：8mm；线规：26AWG+信号放大器。",null,"条",5]
["合计"]
["二、耗材采购信息（协同创新工作室耗材）"]
[1,"串口网关显示屏","8路串口232/485转以太网显示",null,"个",1]
[2,"网络布线制作工具套装","工具一套",null,"套",1]
[3,"护眼台灯","欧普AAA级护眼灯，元睿PRO，白色，双向旋转150度，全光谱Ra98灯珠；",null,"台",6]
[4,"BOW 折叠无线三蓝牙键盘","黑色键盘，蓝牙，触摸可下按，配鼠标，可充电，操作有效范围:10m；可连续工作: ≥30小时；支持系统: ios/Android/Windows；",null,"个",6]
[5,"HDMI转VGA转换器","接口类型:标准HDMI口公头、VGA接口母头；带音频，配电源线，铝合金光银；芯片型号:ITE6693；分辨率:1920*1080P；型号:MM102；线长:16cm；外壳材质:铝镁合金；包装:时尚彩盒",null,"个",5]
[6,"硕方TP66i线号机色带","黑色 TP-R100B",null,"卷",10]
[7,"9V碱性电池","南孚 碱性无汞方形9V电池",null,"粒",30]
[8,"智能播放平台",null,null,"套",1]
[9,"智能调音平台",null,null,"套",1]
[10,"智能送话器",null,null,"套",1]
["合计"]
[]
["合计（耗材采购信息（“双带头人”工作室耗材）、二、耗材采购信息（协同创新工作室耗材））"]
["报价单位名称（公章）：",{"$nulls":3},"报价人：",null,null,"联系电话："]