{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["教学实训中心"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"教学实训中心","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"merged":[[0,0,0,8],[19,1,19,3],[20,1,20,8],[21,0,21,3],[21,4,21,6],[21,7,21,8]],"flags":["formulas_cached_only"]}
["里建校区教学实训综合楼网络接入网络中心机房综合布线工程清单"]
["序号","设备名称","品牌、型号","参数规格","数量","单位","单价（元)","小计（元)","备注"]
[1,"六类非屏蔽网线","AMP六类网线","1、非屏蔽带十字骨架双绞线。兼容所有Cat.6非屏蔽系统，依照ISO/IEC 11801Ed.2；EIA/TIA568；\n2、线缆带宽要求达到350Mhz\n3、芯线直径：≥0.56mm；外径：≥6.3mm",2,"箱"]
[2,"理线架","AMP理线架","AMP理线架",12,"个"]
[3,"水晶头","AMP六类水晶头","AMP六类非屏蔽水晶头",1,"盒"]
[4,"接入交换机","华为 S5720S-28P-LI-AC","24个10/100/1000Base-T以太网端口，4个千兆SFP，交换容量≥300Gbps，包转发率≥50Mpps",11,"台"]
[5,"汇聚交换机","华为 S5720S-28P-SI-AC","24个10/100/1000Base-T以太网端口，4个千兆SFP，交换容量：330Gbps，包转发率≥90Mpps",2,"台"]
[6,"单模光模块","华为单模单纤光模块","SFP-GE-LX-SM1310/1490-BIDI 千兆单模单纤SFP光纤模块\n1、模块类型: SFP\n2、传输距离: 10KM\n3、传输介质: 单模光纤\n4、传输速率：1G b/s\n5、传输波长: 1310nm/1490配对\n6、接口类型: 单LC接口；",8,"个"]
[7,"电模块","华为电口模块","SFP-1000BaseT 光纤口转RJ45电口模块",6,"个"]
[8,"ODF配线架","隆兴 12芯ODF","隆兴 12芯ODF（满配FC耦合器）",2,"台"]
[9,"ODF配线架","隆兴 72芯ODF","隆兴 72芯ODF（满配FC耦合器）",1,"台"]
[10,"光缆","24芯室外光缆","24芯单模室外光纤，采用0.9mm紧套光纤作为中心单元，高模量芳纶纱周边加强；外径小，紧套提供终端直接物理保护；阻燃或不易燃外护套，提供良好的安全保护",300,"米"]
[11,"光缆","12芯室外光缆","12芯单模室外光纤，采用0.9mm紧套光纤作为中心单元，高模量芳纶纱周边加强；外径小，紧套提供终端直接物理保护；阻燃或不易燃外护套，提供良好的安全保护",200,"米"]
[12,"光缆施工费","国标","架空、穿电缆沟",500,"米"]
[13,"光纤熔接","国标","含测试",60,"芯"]
[14,"光缆跳线","D-link","16条3米FC-ＬＣ光缆跳线",16,"条"]
[15,"机柜","三信 9U豪华机柜","三信 9U豪华机挂壁机柜",12,"台"]
[16,"布线辅材","定制","PVC线管、线槽，管卡、胶塞、钢钉、自攻钉、电工胶等",1,"批"]
[17,"设备安装调试","定制","水晶头压制、墙柜安装及交换机供电安装及机柜网线整理，打标记、交换机级联线路布线，含设备搬运、上架、安装及调试等一切人工费。",1,"批"]
[null,"合计：人民币（大写）                                           （¥：       ）"]
["说明","1、本项目报价应包含工程实施过程中的材料、设备、安装调试、人工、运输、机械以及税费等完成项目所需的全部费用。2、施工工期：10个日历日（须在2020年9月10日前完成项目建设并交付验收合格）3、响应文件必须包含报价文件、施工技术方案和营业执照及相关资质材料等正本一份。"]
["报价单位名称：（公章）",{"$nulls":3},"报价人：",null,null,"联系电话："]