{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["办公教学千兆"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"办公教学千兆","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"merged":[[0,0,0,7],[14,1,14,5],[15,0,15,7]],"flags":["formulas_cached_only"]}
["长堽校区办公室网络综合布线清单"]
["序号","设备名称","参数规格","数量","单位","单价（元)","小计（元)","备注"]
[1,"86底盒","86明装底盒",40,"个"]
[2,"罗格朗信息模块","六类RJ45信息模块（含面板及安装）",40,"套"]
[3,"罗格朗六类网线","提供至少155MHZ的信道带宽；支持千兆以太网，线芯规格：无氧铜，导体直径≥0.55mm，含布线安装",1900,"米"]
[4,"罗格朗水晶头","六类水晶头",1,"盒"]
[5,"光端盒","12芯光端盒（配12个FC耦合器）",4,"台"]
[6,"光缆","12芯轻铠装室外光缆，采用0.9mm紧套光纤作为中心单元，高模量芳纶纱周边加强",200,"米"]
[7,"光缆跳线","FC-LC 2米单模跳线",24,"条"]
[8,"光缆敷设","国标",200,"米"]
[9,"光纤熔接","国标，含测试",72,"芯"]
[10," 联塑PVC线槽","PVC：20*10*0.55mm，引入室内线槽，含安装",600,"米"]
[11,"波纹管","阻燃波纹管，含安装",300,"米"]
[12,"三拓机柜ST.6609","9U壁挂网络机柜，高500宽550深450，网络设备安装",3,"台"]
[13,"合计（元）："]
["其它要求：包含交换机、AP设备安装调试、网线布线（穿PP波纹管后放入桥架、桥架及入室内需钻孔）水晶头压制和信息模块安装打线、标签等"]
[]
[null,"报价公司（公司名称):",{"$nulls":3},"联系人：","联系电话："]