{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["装修工程"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"装修工程","index":0,"n_rows":19,"n_cols":16383,"rows_kept":19,"merged":[[0,0,0,6],[18,1,18,4]]}
["水利BIM+虚拟仿真实训室改造项目工程清单"]
["序号","单项名称","工程量","单位","单价（元）","合计（元）","特征及描述"]
["一","实训室装修改造"]
[1,"地面保护",270,"㎡",null,null,"铺牛皮纸保护"]
[2,"墙面刮腻子",380,"㎡",null,null,"两遍腻子"]
[3,"墙面滚涂料",380,"㎡",null,null,"乳胶漆3遍"]
[4,"天花喷涂灰色涂料",282,"㎡",null,null,"乳胶漆电脑配色"]
[5,"生态木格栅吊顶",270,"㎡",null,null,"50*60mm；间距9cm，轻钢龙骨,,8镀锌全螺纹吊杆"]
[6,"窗帘盒制作安装",22,"m",null,null,"白色免漆板"]
[7,"遮光窗帘",22,"m",null,null,"2倍布"]
[8,"长条型灯盘",32,"盏",null,null,"LED光源，40W，铝框，含开关"]
[9,"配电箱",2,"个",null,null,"规格:400*500"]
[10,"小型断路器",14,"个",null,null,"品牌参照正泰同等或高于其品牌，NXB-125 C80 400V-50HZ"]
[11,"电力电缆（从总箱接电）",200,"m",null,null,"YJV22-0.6/1kv-4*16mm2（含安装）"]
[12,"超六类非屏蔽网线及安装",8,"箱"]
[13,"砖砌讲台（2个）",5,"m3",null,null,"6×2米"]
[14,"砖砌讲台贴防滑砖",16,"㎡"]
[15,"材料上楼及垃圾清理",1,"项",null,null,"人工搬运"]
[null,"小计：",{"$nulls":3},{"$f":"SUM(F4:F18)","v":0},{"$nulls":16376},{"$f":"SUM(A19:XFB19)","v":0}]