{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["专用设备购置"],"read":"whole","date_system":"1900"}

{"sheet":"专用设备购置","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"merged":[[0,0,0,6],[1,0,1,3],[1,4,1,6],[18,0,18,5],[19,0,19,6]]}
["购置清单"]
["部门：交通工程学院"]
["序号","货物或项目名称","参考品牌型号规格或配置技术参数","计量单位","数量","单价（元）","合计（元）"]
[1,"四星多频蘑菇头GPS天线","品牌： BROTEX；\n组成：天线+底座+5m长TCN馈线；\n工作电压：DC 3-18V；\n性能参数：能接收GPS、GLONASS、BDS、GALILEO信号。",2,"个"]
[2,"12V100AH金属外壳锂电池","品牌：唤能；\n组成：12V100AH金属外壳锂电池+原装充电器+背包；\n性能参数：\n1.额定电压12V,额定容量100AH；\n2.充电电流5A闪充，峰值放电电池120A；\n3.放电限制电压9.6V，过充保护电压12.6v；",2,"个"]
[3,"微型继电器","SMI－05V-SL-2C系列",200,"个"]
[4,"快速接线端子接线器","按压式快速接线端子CH-2",200,"个"]
[5,"0.75平方汽车导线","汽车电线FLRY-B0.75平方，德标线105度耐温纯铜无氧铜线路改装导线，70米/盘",4,"盘"]
[6,"1.0平方汽车导线","汽车电线FLRY-B1.0平方德标线105度耐温纯铜无氧铜线路改装导线，70米/盘",4,"盘"]
[7,"1.5平方汽车导线","汽车电线FLRY-B1.5平方德标线105度耐温纯铜无氧铜线路改装导线，70米/盘",4,"盘"]
[8,"2.5平方汽车导线","汽车电线FLRY-B2.5平方德标线105度耐温纯铜无氧铜线路改装导线，70米/盘",4,"盘"]
[9,"4.0平方汽车导线","汽车电线FLRY-B4.0平方德标线105度耐温纯铜无氧铜线路改装导线，70米/盘",4,"盘"]
[10,"12V汽车电瓶","风帆蓄电池L2-400 ",4,"个"]
[11,"HDMI无线投屏器","HDMI无线投屏器，型号QRT-AA1，主机+发射器+HDMI高清线",4,"套"]
[12,"24GHZ毫米波雷达","型号：SP25，短距广角工业雷达，探测距离30M，推测广角100度，超低功耗0.5w",2,"个"]
[13,"激光雷达","思岚激光雷达，型号为RPLIDAR A1",2,"个"]
[14,"远程4G摄像头","内存容量64GB，4G+WIFI一路，清晰度为5MB，焦距为2.8mm",2,"个"]
[15,"远程4G摄像头","品牌: HIKVISION/海康威视,型号：DS-U12，像素：400万像素；\n组成：3.6mm摄像头+2M接线（USB2.0接口）",2,"个"]
["总计金额（元）："]
["一、其他要求:\n    \n\n\n"]
[]
[null,"报价公司（公司名称）：",null,"联系人：",null,"联系电话："]