{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":136,"n_cols":7,"rows_kept":136,"merged":[[0,0,0,6],[136,1,136,6]],"flags":["formulas_cached_only"]}
["2020年春季学期汽车实训耗材采购清单"]
["序号","货物或项目名称","参考品牌型号规格或配置技术参数","计量单位","数量","单价（元）","合计（元）"]
["1","无损探针","1.0mm针头测试探针，带4mm香蕉插座（黑红两色）","枚",70]
["2","测试线","1米香蕉插头转鳄鱼夹","根",30]
["3","鳄鱼夹","黑色大号（45MM）","个",50]
["4","鳄鱼夹","红色大号（45MM）","个",50]
["5","2进2出快速接线端子连接器","品牌：CCZJ/正继\n型号： PCT-222\n技术规格：适用多股软线0.08-2.5mm2\n         适用单股硬线0.08－4.0mm2","个",100]
["6","2孔快速接线端子连接器","品牌：CCZJ/正继\n型号： PCT-212\n技术规格：适用多股软线0.08-2.5mm2\n         适用单股硬线0.08－4.0mm2","个",100]
["7","插拔式尼龙子弹型公母对接端子快速连接器","品牌：CCZJ/正继\n型号：NZTD0.5-50T\n技术规格：0.3-1.0mm2","套",100]
["8","插拔式尼龙子弹型公母对接端子快速连接器","品牌：CCZJ/正继\n型号： NZTD1.0-30T\n技术规格：0.5-1.5mm2","套",100]
["9","汽车电线改装线电路专用耐高温纯铜加粗国标电源线车用线束(60米一盘)","国标紫铜线\n规格：0.75mm2\n颜色：棕色","米",60]
["10","汽车电线改装线电路专用耐高温纯铜加粗国标电源线车用线束(60米一盘)","国标紫铜线\n规格：1.0mm2\n颜色：棕色","米",60]
["11","汽车电线改装线电路专用耐高温纯铜加粗国标电源线车用线束(60米一盘)","国标紫铜线\n规格：1.5mm2\n颜色：棕色","米",60]
["12","汽车电线改装线电路专用耐高温纯铜加粗国标电源线车用线束(60米一盘)","国标紫铜线\n规格：0.75mm2\n颜色：红色","米",60]
["13","汽车电线改装线电路专用耐高温纯铜加粗国标电源线车用线束(60米一盘)","国标紫铜线\n规格：1.0mm2\n颜色：红色","米",60]
["14","汽车电线改装线电路专用耐高温纯铜加粗国标电源线车用线束(60米一盘)","国标紫铜线\n规格：1.5mm2\n颜色：红色","米",60]
["15","丰田卡罗拉继电器","型号：T90987-T2005  规格：12V 30A","个",40]
["16","丰田卡罗拉继电器","型号：T90987-T2004  规格：12V 30A","个",20]
["17","大众速腾645继电器","型号：大众4RA007791-20  规格：12V 40A","个",40]
["18","水泥电阻","规格：5瓦  10欧姆","个",1]
["19","水泥电阻","规格：5瓦   20欧姆","个",1]
["20","水泥电阻","规格：5瓦   100欧姆","个",1]
["21","水泥电阻","规格：10瓦   10欧姆","个",2]
["22","汽车保险插片","7.5A（17款卡罗拉）100片/盒","盒",5]
["23","汽车保险插片","10A（17款卡罗拉）100片/盒","盒",5]
["24","汽车保险插片","15A（17款卡罗拉）100片/盒","盒",5]
["25","汽车保险插片","20A（17款卡罗拉）100片/盒","盒",5]
["26","电工绝缘胶带","3M ","卷",50]
["27","耐高温绒布胶带","25mmx50m（宽x长）","卷",4]
["28","热缩管带","汽车电线用热缩三倍，直径2.4","米",10]
["29","热缩管带","汽车电线用热缩三倍，直径3.2","米",10]
["30","热缩管带","汽车电线用热缩三倍，直径4.8","米",10]
["31","汽车接线器","1P连接头带线  12V  ","个",5]
["32","电线扎带","8X300mm（100条/包）","包",5]
["33","速腾卡罗拉全车卡扣","成套","套",4]
["34","双头鳄鱼夹测试线","中号","根",40]
["35","保险丝夹","汽车中号保险丝取拔夹子","个",10]
["36","手电筒","康铭KM-8911","个",8]
["37","汽车维修工作灯","卡里忒斯X303plus充电款，内置18650可充电锂电池；600流明可旋转侧灯；500流明主灯","个",8]
["38","继电器","吉利EV300车型使用，30A12VDCAR0807F2","个",20]
["39","继电器","吉利EV300车型使用，40A12VDCAR0927B1","个",20]
["40","继电器","吉利EV450车型使用","个",20]
["41","保险","吉利EV300车型使用，至少包含7.5A、10A、15A、20A、30A","盒",5]
["42","保险丝夹","汽车小号保险丝取拔夹子","个",10]
["43","保险丝夹","汽车迷你保险丝取拔夹子","个",10]
["44","电池","2号，1.5V，绝缘测试仪用","节",30]
["45","万能电路板","9×12cm","块",1000]
["46","万能电路板","5×6cm","块",500]
["47","普通发光二极管","普通型，直径为Φ5mm，红色3v","只",2000]
["48","普通发光二极管","普通型，直径为Φ5mm，绿色3v","只",2000]
["49","普通整流二极管","1A硅整流二极管","只",2000]
["50","  普通稳压管","12V/1A","只",500]
["51","电解电容","10uF/25V","只",500]
["52","电解电容","100uF/25V","只",500]
["53","普通小功率三极管","NPN型","只",500]
["54","微调电阻","100K","只",500]
["55","微调电阻","1M","只",500]
["56","微调电阻","2M","只",500]
["57","普通电阻","20欧、1/4瓦","个",1000]
["58","普通电阻","80欧、1/4瓦","个",1000]
["59","普通电阻","200欧、1/4瓦","个",1000]
["60","普通电阻","3K、1/4瓦","个",1000]
["61","普通电阻","200K、1/4瓦","个",1000]
["62","普通电阻","20欧、1瓦","个",1000]
["63","普通电阻","200K、1瓦","个",1000]
["64","光敏电阻","5506型5mm","只",500]
["65","     集成电路","555时基（带座）","套",500]
["66","细导线","纯铜0.5平(100米/卷）","卷",6]
["67","排插","新国标公牛五插5米插排2500w","个",40]
["68","插头","10A扁角2相插头","只",20]
["69","制冷剂","R134a（金冷牌）250ml","瓶",100]
["70","连杆螺栓","帕萨特b5发动机2.0","个",32]
["71","活塞环","帕萨特b5发动机2.0","套",4]
["72","连杆","帕萨特b5发动机2.0","组",1]
["73","进排气门","帕萨特b5发动机2.0","副",2]
["74","曲轴大小轴瓦","帕萨特b5发动机2.0（0.00号）","套",2]
["75","油底壳螺栓","帕萨特b5发动机2.0","颗",20]
["76","前后油封螺栓","帕萨特b5发动机2.0","颗",20]
["77","连杆螺栓","帕萨特b5发动机2.0","颗",20]
["78","塑性线间隙规","PL-A，0.025~0.175mm（100条/盒）","盒",4]
["79","凸轮轴轴承盖螺栓","帕萨特b5发动机2.0","颗",20]
["80","主轴承盖螺栓","帕萨特b5发动机2.0","个",32]
["81","密封胶","卡夫特","支",40]
["82","发动机润滑机油","10-W30，4L装","桶",20]
["83","化油器清洗剂","3M ","瓶",20]
["84","柏油清洗剂","车仆500g","瓶",50]
["85","除锈剂","车仆270ml","瓶",30]
["86","正时皮带","帕萨特b5发动机2.0","条",9]
["87","水泵皮带","帕萨特b5发动机2.0","条",9]
["88","楔形皮带","帕萨特b5发动机2.0","条",9]
["89","螺丝分类收纳盒","24格箱442*310*75","个",8]
["90","楔形带轮（减振器）螺丝","帕萨特b5发动机2.0","个",32]
["91","标签贴纸","不干胶贴纸19x28mm/枚，每张40枚一包共50张","包",8]
["92","空调滤清器","2017款1.4T速腾；符合实训要求。","个",6]
["93","耐油绝缘胶垫","厚度：6mm，外形尺寸：1100*650*6（mm）。","张",20]
["94","蓄电池蒸馏水","高纯度蒸馏水，1.9L。","瓶",4]
["95","电解液原液","比重1.28电解液原液1箱（2Lx6瓶）","箱",1]
["96","油管气管卡箍","304不锈钢，直径6-12mm","个",50]
["97","油管气管卡箍","304不锈钢，直径13-19mm","个",50]
["98","油管气管卡箍","304不锈钢，直径19-29mm","个",50]
["99","油管气管卡箍","304不锈钢，直径78-101mm","个",50]
["100","油管气管卡箍","304不锈钢，直径105-127mm","个",50]
["101","去污液蜡","车仆330ml去污液蜡","瓶",20]
["102","标准气体","南华五气体尾气分析仪标准气体","瓶",16]
["103","门板内饰撬板","好美36件套 HM-3698","套",8]
["104","手电钻","Bosch/博世GSB120-LI多功能手电钻（双锂电池）","套",3]
["105","钻头批头","博世33件套装2607019325（含冲击钻头麻花钻头批头）","套",3]
["106","免驱USB无线网卡","TP-LINK免驱动双频usb无线网卡WDN5200H传输速率600Mbps","个",10]
["107","一次性口罩（50个/包）","保护康无纺布4层独立包装一次性口罩（50个/包）","包",10]
["108","地毯","红色，2米*12米","张",4]
["109","示波器电池","BTHP101","个",2]
["110","洗手粉 ","洁立净（420g/罐，30罐/箱）","箱",10]
["111","塞尺","世达09405不锈钢塞尺（0.01—1.00mm）","把",12]
["112","汽车镀膜剂","帕睿纳水磨密封剂300ml","套",10]
["113"," 汽车美容海绵","帕睿纳进口镀膜专用海绵去污去垢海绵","块",30]
["114","打蜡毛巾","帕睿纳高低长短毛毛巾40*40","条",20]
["115","擦车毛巾","帕睿纳珊瑚绒毛巾40*40","条",20]
["116","高泡洗车液","樱桃20L","桶",2]
["117","软毛伸缩拖把","长柄伸缩软毛9米","把",4]
["118","汽车除尘刷子","短柄纯棉","把",4]
["119","洗车海绵","特大号流沙型","个",12]
["120","轮毂刷子","清洗车轮专用软毛钢圈刷子","把",5]
["121","洗车毛巾","大号200cm*60cm加厚超细纤维","条",8]
["122","洗车毛巾","小号加厚超细纤维42cm*26cm","条",30]
["123","抹布","纯棉抹布","斤",50]
["124","帕萨特大修包","帕萨特b5发动机2.0","套",20]
["125","车身保养四件套","德国wurth伍尔特，原装","套",20]
["126","左前车窗升降总开关","大众迈腾B8L1.8","个",1]
["127","外后视镜开关（带折叠）","大众迈腾B8L1.8","个",1]
["128","一键启动开关","大众迈腾B8L1.8","个",1]
["129","活塞环卡钳","开口40-100mm","个",8]
["130","喷枪","特威C71喷枪套装（特威C71上壶1.5口径喷枪一把，600CC喷壶一个，枪架一个，过滤器一个，调压表一个，滤网两个）","套",3]
["131","启停蓄电池","大众迈腾B8L1.8瓦尔塔EFB70AH","个",1]
["132","喷枪","深田5000b上壶1.3口径喷枪套装（深田5000B1.3口径喷枪一把，600CC喷壶一个，3M口罩一个，调压表一个，过滤器一个，吹枪一把，快接头一个，滤网两个，枪架一个）","套",3]
[]
[null,"合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}