{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Chart3","Chart2","Chart1","Sheet1 "],"not_rendered":{"charts":3,"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Chart3","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Chart2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Chart1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet1 ","index":3,"n_rows":15,"n_cols":7,"rows_kept":15,"merged":[[0,0,0,6],[2,0,2,6],[6,0,6,1],[7,0,7,6],[13,0,13,1],[14,0,14,1]],"flags":["formulas_cached_only"]}
["广西水利电力职业技术学院食堂更换不锈钢水沟盖板项目清单"]
["序号","单项名称","工程量","单位","单价（元）","合计（元）","特征及主要功能要求描述"]
["一、长堽校区思源轩食堂一楼更换不锈钢水沟盖板"]
[1,"清除长堽思源轩食堂原有水沟盖板",{"v":1,"d":"1.00"},"项"]
[2,"定制304多孔不锈钢盖板",{"v":50,"d":"50.00"},"块",null,null,"400*500；304不锈钢材质，厚度1.2，冲孔盖板"]
[3,"垃圾清理",1,"项"]
["本项小计"]
["二、里建校区知味轩饭堂更换不锈钢水沟盖板"]
[1,"清除里建知味轩食堂原有水沟盖板",{"v":1,"d":"1.00"},"项"]
[2,"食堂一楼定制304多孔不锈钢盖板",{"v":371,"d":"371.00"},"块",null,null,"400*500；304不锈钢材质，厚度1.2，冲孔盖板"]
[3,"食堂二楼定制304多孔不锈钢盖板",{"v":340,"d":"340.00"},"块",null,null,"400*500；304不锈钢材质，厚度1.2，冲孔盖板"]
[4,"食堂三楼定制304多孔不锈钢盖板",{"v":162,"d":"162.00"},"块",null,null,"400*500；304不锈钢材质，厚度1.2，冲孔盖板"]
[5,"垃圾清理",1,"项"]
["本项小计"]
["一、二项合计"]