{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"merged":[[0,0,0,6],[10,0,10,6],[11,1,11,6],[12,0,12,1]]}
["红色文化教育馆文化墙及走廊格栅吊顶建设清单"]
[]
["序号","单项名称","特征及描述","单位","工程量","单价（元）","合计（元）"]
[1,"拆除原侧墙展板","拆除原文化墙的红色教育展板；尺寸：10.55mX2.84mX2个；","㎡",59.92]
[2,"墙面修复","拆除后的墙壁损伤，用腻子乳胶漆进行修复；尺寸：10.55mX2.84mX2个；","㎡",59.92]
[3,"文化墙制作","采用 PVC 材质制作一片图片及字体，设计一些造型；展示红色文化的内容。根据现场及室内主题风格进行整体设计；图片及方案待采购人确认后方可制作安装；10.55mX2.84mX2个；","㎡",59.92]
[4,"拆除LED屏两侧的白色字体","对LED屏两边的白色字体进行拆除，拆除后底层铝塑板胶水会损坏或污染，需重新更换；高3.5X宽1米X2个；","㎡",{"v":7,"d":"7.00"}]
[5,"更换教室后墙灯箱广告图片","拆除原灯箱广告表面的软膜，更换自选供业主确认或者由业主单位选定的图案，重新安装；材质：专用灯箱软膜；8.4mX3.4mX2个","㎡",57.12]
[6,"走廊格栅吊顶","红色文化馆及旁边办公室门前走廊顶部，做格栅吊顶；铝合金材质格栅，厚度0.4mm；宽5公分，间距7公分；","㎡",{"v":76,"d":"76.00"}]
[7,"格栅灯及配线、管等","条形格栅灯长度28W-1200mmX10mm；及150米电源线WDZ-BYJ-2.5；、PVC-25管50米等","套",{"v":6,"d":"6.00"}]
["合计:人民币（大写）                                                （¥：             ）"]
["商务要求","1、报价应包含材料、设计、制作安装、人工、运输、机械以及税费等完成本项目所需的全部费用。\n2、交货期：10个日历日。采购需求如有不明之处，请咨询项目联系人：江老师13978621558\n3、有意向竞标的单位，请在2020年11月19日上午11:00前将报价文件盖章后扫描成pdf文件发送到gxsdxyzcgl@163.com"]
["报价单位（公章）：",null,null,"报价人：",null,"联系电话："]